Notes:

!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
If a version prior to 0.6.12 is installed on the GMR6K, the GMR6K
CAN ONLY be updated using the J-Link debugger.
This is due to internal memory map changes for where the bootloader
and the primary are in the stored Kinetis CPU.
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!

Version 0.6.15 and later is required for GMR6K BC-00560 rev 2.0.E PCB.

UpdateUtilityUser.exe can be used to update the firmware in a GMR6000.
Firmware for other products is not included in this distribution.

Use the copy of Windiscovery and UpdateUtility included in this beta release folder

This version of Windiscovery and the UpdateUtility will not work correctly with previous versions
of GMR6K firmware. It is compatible with legacy products (GMR1000,
GMR5000, clocks, etc.).

Command line options for UpdateUtility and Windiscovery:

-randomport
-engineering
-production
-nomacverify (UpdateUtility only)

logging features:
 -logging -logconsole -loglevel=3

Built using:

branch: tip of development
tag: 1.0.5_release_dev
1/8/2026 commit 3187c2

